
1. Flash tool option, please select as picture shows below:

Select USB download

Select Format FAT auto

Select backup and restore as no action



1. When download, click download button, plus USB cable, then press “\*” key on mobile phone, then plus battery, keep press “\*” key till flash tool screen display the blue status bar, then release “\*” key. Wait till download finish.


For the new samples, 2pcs, because they already have right radio parameters and with old V8 software, if you want to update to new V8 software,(Of course also they are no need to update to new V8 software because they already has right radio paramters). The download method is as follow:

1. Flash tool, please use the one which I sent you today, version is 5.1152.
2. Software version: Please use the new V8 software which I sent to you today.
3. Flash tool option, please select as picture shows below:

Select USD download

Select Format FAT auto

Select backup and restore as backup—D/L and format—Restore



1. When download, click download button, plus USB cable, then keep to press “\*” key on mobile phone, then plus battery, keep press “\*” key till flash tool screen display the blue status bar, then release “\*” key. **Wait when the blue status bar almost finished, then press “\*” key again, then keep pressing until display green “O” to show download finish. (The last step to keep press “\*” key is for restore the radio calibration parameters.)**